{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":7,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[[6,0,6,9],[7,0,7,9],[18,5,18,8],[16,0,16,9],[9,1,9,8]]}
["項目","VBA計算"]
["X座標(m)",-659711.34510000004]
["Y座標(m)",-107087.44070000001]
["地盤高(m)",19.444500000000001]
[]
[]
[]
[]
[null,"入力欄"]
["GGAデータ","$GNGGA,045154.00,2702.64343,N,12825.23572,E,4,12,0.89,23.7,M,29.0,M,1.0,0495*52"]
["平面直角座標系",1]
["アンテナ高(m)",1.87]
[]
[]
[]
["本VBAマクロは入力欄に入力された　GGA、平面直角座標系番号、アンテナ高より、平面直角座標XYと地盤高を計算します。"]
["国土地理院のAPI（Application Programming Interface）を利用しますから、インターネットに接続してください。"]
["CLAS Androidアプリでトラブルがあった時は、KabutoDynaEXE をお使いください。"]
[null,null,null,null,null,"2025/08/28　Ryoji Tanaka"]